**TANGLED FEET and HALF MOON THEATRE present**

**NEED A LITTLE HELP**

**TECHNICAL REQUIREMENTS**

**Configuration:**

The show is performed in traverse with a central performance carpet of 7m x 3.2m with an audience area on each side. The performance area is carpet, and the audience space consists of rugs and cushions. Additional seating may be added along the back of the audience space. There are pieces of wooden set at either end of the performance space. One piece of set has a doorway within it. This should be situated closest to where the audience enter.

The minimum size of space we need is 10m in length and 6.5m wide.

We need height of 3m approx.

Audience size: 80 maximum.

**Logistics:**

The performance is45mins. We can do two shows a day with a break of 2 hours between the end of one and start of another, the set stays in place between shows. Whilst we can share the space between the first and second show we need an empty space 30 minutes before second show to prepare.

**Get In:**
1.5 hrs from clean, empty space, once van is unloaded and all set is in space, please allow time to unpack van (45 mins)

**Get Out:**
45mins once audience have left

**Parking:**

One LWB Van

**Lighting:**

The show has been designed to work in any space. We require 12 LED parcans in total. 3 at each corner of the performance space on stands. (if operating in a theatre space – these could be moved to overhead if necessary.) These work as colour boosters to a general light which can be daylight, normal room lights, or a warm general cover if performed in a theatre space. We bring our own ETC Nomad system for control, and need a DMX Feed at our operating position.

**Sound:**

Sound is played back from a MacBook or an iPad. We require a PA system suitable for your space. Ideally we would be able to place a speaker at each corner of the performance area, but we can work with two speakers placed as per the diagram below. We need a minijack input and a sound desk at our operating position.

**Operating position:**

We need a small table for our operating position which will be place in the space at the opposite end to the audience entrance. This will hold the sound desk and two laptops. We will need power to this position.

 